Name
EfiLdrImage.exe Options PE1 PE2 PE3 …
Synopsis
EfiLdrImage.exe [-v | -q | -d] -o <FileName> <InputFile1> [<inputfile2>]…
EfiLdrImage.exe –h
EfiLdrImage.exe --version
Description
The EfiLdrImage tool is used to combine PE files into EFILDR image with Efi loader header.
Options
If no options are specified, tool prints usage.
-o, --output Filename
	The file that contains the combined loader file.
--version
	Print version and copyright of this program and exit
-v, --verbose
Turn on verbose output with informational messages printed. This is a count value, so specifying –vv can be used to increase the verbosity level.
-q, --quiet
	Disable all messages except FATAL ERRORS
-d, --debug [#]
	Enable debug messages, at level #
-h, --help
	Print copyright, version and usage of this program and exit
Status codes returned
STATUS_SUCCESS 	0	The action was completed as requested.	
STATUS_ERROR 		2	The action failed.	

Example
1. c:\Tools\EfiLdrImage.exe –o loader.img loader.data loader1.data
The loader.data and loader1.data will be put into loader.img file which contains a EFI loader header.
Bugs
No known issues
Files 
None.
See also
 None.
License
Copyright (c) 1999 - 2011, Intel Corporation. All rights reserved.
This program and the accompanying materials are licensed and made available 
under the terms and conditions of the BSD License which accompanies this 
distribution.  The full text of the license may be found at
http://opensource.org/licenses/bsd-license.php

THE PROGRAM IS DISTRIBUTED UNDER THE BSD LICENSE ON AN "AS IS" BASIS,WITHOUT WARRANTIES OR REPRESENTATIONS OF ANY KIND, EITHER EXPRESS OR IMPLIED.